ASSIGNMENT 4

|  |  |
| --- | --- |
| **Date** | 29 Oct 22 |
| **Name** | Pradeeprajan R |
| **Team ID** | PNT2022TMID17711 |
| **Project Name** | Smart Waste Management For Metropolitan Cities |

Write code and connections in wokwi for ultrasonic sensor.

Whenever distance is less than 100 cms send "alert" to ibm cloud and display in device recent events.

Upload document with wokwi share link and images of ibm cloud

# CODE:

#include <WiFi.h>

#include <PubSubClient.h> WiFiClient;

#define ORG "nhpwjc"

#define DEVICE\_TYPE "NodeMCU" #define DEVICE\_ID "USE YOUR ID" #define TOKEN "USE YOUR TOKEN"

#define speed 0.034

char server[] = ORG ".messaging.internetofthings.ibmcloud.com"; char publishTopic[] = "iot-2/evt/Data/fmt/json"; char topic[] = "iot-2/cmd/home/fmt/String"; char authMethod[] = "use-token- auth"; char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

PubSubClient

publishData();

client(server,

1883, wifiClient); void

const int trigpin=5;

const int echopin=18; String command; String data="";

long duration; float dist;

void setup()

{

**Serial**.begin(115200); pinMode(trigpin, OUTPUT);

pinMode(echopin, INPUT); wifiConnect(); mqttConnect();

} void loop() { publishData(); delay(500);

if (!client.loop()) { mqttConnect();

}

}

void wifiConnect() {

**Serial**.print("Connecting to "); **Serial**.print("Wifi"); WiFi.begin("Wokwi-GUEST", "", 6); while (WiFi.status() != WL\_CONNECTED) { delay(500);

**Serial**.print(".");

}

**Serial**.print("WiFi connected, IP address: "); **Serial**.println(WiFi.localIP());

}

void mqttConnect() { if (!client.connected()) {

**Serial**.print("Reconnecting MQTT client to "); **Serial**.println(server); while (!client.connect(clientId, authMethod, token)) { **Serial**.print("."); delay(500);

}

initManagedDevice(); **Serial**.println();

} }

void initManagedDevice() { if (client.subscribe(topic)) {

// Serial.println(client.subscribe(topic)); **Serial**.println("subscribe to cmd OK");

} else {

**Serial**.println("subscribe to cmd FAILED"); } } void publishData()

{ digitalWrite(trigpin,LOW); digitalWrite(trigpin,HIGH);

delayMicroseconds(10); digitalWrite(trigpin,LOW); duration=pulseIn(echopin,HIGH); dist=duration\*speed/2; if(dist<100){

String payload = "{\"Alert distance\":"; payload += dist;

payload += "}"; **Serial**.print("\n"); **Serial**.print("Sending payload: "); **Serial**.println(payload);

if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish OK");

} else {


**Serial**.println("Publish FAILED");

}



}

}

# CONNECTIONS:



**OUTPUT:**



**WOKWI LINK -https://wokwi.com/projects/345395196387656275**